Single / Double bottle cabinet



Technical Parameter

|  |  |  |  |
| --- | --- | --- | --- |
| Model | Specification | LXWXH | Product description |
| Single - bottle cabinet  | 40/70L | 500X500X1450 | The cabinet is divided into two types : assembly and welding; the thickness of the assembly plate is 1.2mm; welding plate thickness is 1.0mm; the box shape, size can be customized  |
| 90L | 500X500X1600 |
| 120L | 500X500X1900 |
| 150L | 550X520X1900 |
| 180L | 550X520X2100 |
| Double - bottle cabinet | 40/70L | 500X900X1450 |
| 90L | 500X900X1600 |
| 120L | 500X900X1900 |
| 150L | 550X1000X1900 |
| 180L | 550X1050X2100 |